CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.1pl6/conf/instr/spect/uxnmr.info
Date         : Tue Apr 24 14:12:06 2018
Release      : TopSpin Acquisition Version 3.1-pl6
Installed in : C:/Bruker/TopSpin3.1pl6
Host         : AMRGROB441SKR
OS           : Windows 7 (Vs 6.1)
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 2533 MHz)
User         : AMER\FCNGRO-BRKOA
Description  : Avance III 400
Location     : 
System       : Avance III NMR spectrometer
1H-frequency : 399.72 MHz
Order Number : 
Configured in: C:/Bruker/TopSpin3.1pl6/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
- Tctrl : 1
- Fctrls: 2
- Gctrl1: without digital preemphasis
- Rctrl : 1
- FREDs : none
- DPP : none

DRU: AQS DRU Z100977/01632 ECL 06.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 120516
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x72   0x4    AV  R  5.0 REC-1  AQS RXAD400 Z102116/2187 ECL 05.00
     3   0x34  0x2   0x1        X  5.2 REF-1  REF-400 Reference Board for AQS Receiver
     4   0x24 0x11   0x8    AD  S  2.6 SGU-1  AQS SGU/2 400 Z103080/02749 ECL 02.06 FPGA-Vs=AE
     5   0x25 0x11   0x8    AD  S  2.6 SGU-2  AQS SGU/2 400 Z103080/02750 ECL 02.06 FPGA-Vs=AE
     8   0x36  0x5     0        A  7.0 BLA-1  BLA2BB 150/60 20-400 W1345049/2686 ECL 7
    --   0x20 0xd7     0        B  0.1 MASTER AVANCE Console NB-E Wired V2
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: 1 AQS-Minirouter

Amplifiers (AQS configuration):
  RO  Amplifier  Module  Nucleus  Power/W  Switchbox Name PN/SN/FW
   1      1         1        B      150    N         BLA2BB 150/60 20-400 W1345049/2686/-
   2      1         2        B       60    N         BLA2BB 150/60 20-400 W1345049/2686/-


Transmitters at the spectrometer subnet:
----------------------------------------
LTRX Z109888/00494 ECL 03.00:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 400: Z109888/00494 ECL 03.00

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20101206
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 20
- Shim System = BOSS1-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 400: Z109888/00494 ECL 03.00
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/00364 ECL 02.03
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/00414 ECL 01.02

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Automatic Changer: device connected to 149.236.99.254:/dev/tty04
- Capacity: 60 holders
- Firmware: 20150813
- use BACS air  = yes
- BACS sx delay = 0 s
- Sample Rail fast changer mode = no

Sample Changers at the spectrometer subnet:
-------------------------------------------
 - BACS2_H15000_0091: at TCP/IP address 149.236.99.251


Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: no LED display for tuning and matching
    Module  1 : 1H/2H 1H (virtual 50 Ohm reference: 274.8%/92.8deg)
                 PN=Z003951, SN=00562 from 20110223
    Module  2 : 1H/2H 2H (virtual 50 Ohm reference: 101.6%/-67.2deg)
                 PN=Z003951, SN=00562 from 20110223
    Module  3 : XBB19F 2HS
                 PN=Z003955, SN=00571 from 20110217


Frequency generation:
- F1: for SGU
- F2: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 2 of transmitter 1 (BLA2BB 150/60 20-400 W1345049/2686)
SGU1 AUX  output -> input 1 of transmitter 2 (BSMS/2 LOCK TRANSCEIVER 400 Z109888/00494 at TCP/IP 149.236.99.20)
SGU2 NORM output -> input 3 of transmitter 1 (BLA2BB 150/60 20-400 W1345049/2686)
SGU2 AUX  output -> TUNE signal input of HPPR

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLA2BB 150/60 20-400 W1345049/2686) amplifier B-150W uses blanking 1
transmitter 1 (BLA2BB 150/60 20-400 W1345049/2686) amplifier B-60W uses blanking 2
transmitter 2 (BSMS/2 LOCK TRANSCEIVER 400 Z109888/00494 at TCP/IP 149.236.99.20) amplifier 2H-5W uses blanking 3

