CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.2.6/conf/instr/spect/uxnmr.info
Date         : Fri Apr  1 14:35:23 2016
Release      : TOPSPIN Version 3.2-pl6
Installed in : /opt/topspin3.2.6
Host         : CZC10591BX
OS           : CentOS release 5.6 (Final)
CPU          : Intel(R) Xeon(R) CPU W3565 @ 3.20GHz (4 cores at 1596 MHz)
User         : nmrsu (NMR Administrator (nmrsu))
Description  : Avance-AV 500
Location     : AstraZeneca Cambridge, Darwin Building
System       : Avance-AV NMR spectrometer
1H-frequency : 500.13 MHz
Order Number : 
Configured in: /opt/topspin3.2.6/conf/instr/spect

#--------------------
#  FCU configuration:
#--------------------
board # 1 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 2 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)

DRU: AQS DRU-E Z102520/00063 ECL 00.01
- TCP/IP address = 149.236.99.89
- Firmware Version = 150604

Gcu: GCU3_SlowIF

AQS: connected to spect:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x2    AW  R  1.1 REC-1  AQS RXAD600 Z102117/46 ECL 1.01
     3   0x34 0xc0   0x1        X  0.4 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x18   0x4    BH  S  3.0 SGU-1  AQS SGU600 Z003831/01785 ECL 3.0
     5   0x25 0x18   0x4    BH  S  3.0 SGU-2  AQS SGU600 Z003831/01777 ECL 3.0
     8   0x3c  0x4     0        Y  1.0 ROUT-1 Avance Router 3/5
    21   0x21  0xa     0        P  1.0 PSD-1  Power Supply Distribution Board
    25   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: 1 Avance-Router

Amplifier Control Board:  connected to spect:/dev/tty20


Amplifiers (ACB configuration):
  RO  Amplifier  Module  Nucleus  Power/W  Switchbox Name PN/SN/FW
   1      1         1        X      300    Y  (V=de) BLAXH 300/100 W1345062/-/20071205
   2      1         2       1H      100    Y  (-""-) BLAXH 300/100 W1345062/-/20071205
   3      2         1       2H       20    N         BSMS 2HTX -/-/-



- Type: BSMS/1
- absolute lockshift frequency =  13227000 Hz
- 2HTX Amplifier: connected to router output 3
- GAB type = GAB
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)

Bruker Automatic Changer: device connected to spect:/dev/tty08
- Capacity: 120 holders
- Firmware: 20040805
- use BACS air  = yes
- BACS sx delay = 10 s
- Sample Rail fast changer mode = no

Lock: device connected to spect:/dev/tty04

Eurotherm VTU: device connected to spect:/dev/tty05

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to spect:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                 PN=Z003461, SN=00395 from 20050106
    Module  2 : XBB19F 2HS
                 PN=Z003505, SN=00417 from 20041207
    Module  3 : 2H
                 PN=Z003472, SN=00403 from 20041202
    Module  4 : QNP Function Module


Frequency generation:
- F1: for SGU
- F2: for SGU



