
New TopShim run:

version = topshim 2.0.0
date = 2022-06-03
time = 10:43:31.310
command = topshim 

1D SHIMMING

Parameters:

maximum order = 5
probe = Z163739_0080
solvent = CDCl3
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 7.24 ppm
optimisation parameters = ls
linewidth 1H = 0.10 Hz
envelope shape / strictness = 2.00 / 200

Results:

initial B0 stdDev = 11.15 Hz
sample size = 2.93 cm, position = 0.03 cm
final B0 stdDev = 0.20 Hz > improvement = 55.9
envelope width = 0.46 Hz
shim changes: 
Z	+286
Z2	-79
Z3	+38
Z4	-89
Z5	+34

duration = 1 min 16 sec
completed successfully
finished Fri Jun  3 10:44:45 2022


========================================================================
