
New TopShim run:

version = topshim 2.0.0
date = 2021-06-16
time = 11:32:18.008
command = topshim 

1D SHIMMING

Parameters:

maximum order = 5
probe = Z163739_0080
solvent = CDCl3
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 7.24 ppm
optimisation parameters = ls
linewidth 1H = 0.10 Hz
envelope shape / strictness = 2.00 / 200

Results:

initial B0 stdDev = 5.87 Hz
sample size = 2.87 cm, position = 0.03 cm
final B0 stdDev = 0.50 Hz > improvement = 11.7
envelope width = 2.07 Hz
shim changes: 
Z	+11
Z2	-89
Z3	+52
Z4	-235
Z5	+140

duration = 1 min 20 sec
completed successfully
finished Wed Jun 16 11:33:35 2021


========================================================================
