
New TopShim run:

version = topshim 2.1.0
date = 2023-05-30
time = 22:37:28.162
command = topshim 

FINE SHIMMING

Parameters:

probe = Z154039_0001
solvent = CDCl3
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 7.24 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 3.1 Hz, Target= 0.4 Hz, After= 0.3 Hz
Iteration 2: FWHM Before= 0.3 Hz, Target= 0.3 Hz, After= 0.6 Hz
Iteration 3: FWHM Before= 0.6 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration 4: FWHM Before= 0.4 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration 5: FWHM Before= 0.4 Hz, Target= 0.3 Hz, After= 0.3 Hz
Iteration 6: FWHM Before= 0.3 Hz, Target= 0.3 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.329

shim changes: 
Z	-339
Z2	-47
Z3	+24
Z4	-27
Z5	-196
Z6	-833
Z7	+2270
Z8	+5888

duration = 1 min 46 sec
completed successfully
finished Tue May 30 22:39:12 2023


========================================================================
