CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.6.4/conf/instr/AV600/uxnmr.info
Date         : Tue Aug 08 12:42:43 2023
Release      : TopSpin 3.6.4
Installed in : C:/Bruker/TopSpin3.6.4
Host         : TOPSPIN3
OS           : Windows 7 Professional (Vs 6.1)
CPU          : Intel(R) Xeon(R) CPU E5-1620 0 @ 3.60GHz (8 cores at 3591 MHz with Hyperthreading)
User         : Cryotool
System       : Avance III 600 NMR spectrometer
1H-frequency : 600.13 MHz
Description  : Avance III 600
Location     : Department of Chemistry, University College London
Bruker Order : GH001707
Configured in: TOPSPIN3:C:/Bruker/TopSpin3.6.4/conf/instr/AV600

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.252
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/01011 ECL 04.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x4    AW  R  4.2 REC-1  AQS RXAD600 Z102117/486 ECL 04.02
     3   0x34 0xc0   0x1        X  2.0 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x19   0x8    AE  S  2.1 SGU-1  AQS SGU/2 600 Z103081/00799 ECL 02.01 FPGA-Vs=AF
     5   0x25 0x19   0x8    AE  S  2.1 SGU-2  AQS SGU/2 600 Z103081/00792 ECL 02.01 FPGA-Vs=AF
     6   0x26 0x19   0x8    AE  S  2.1 SGU-3  AQS SGU/2 600 Z103081/00780 ECL 02.01 FPGA-Vs=AF
     7   0x27 0x19   0x8    AE  S  2.1 SGU-4  AQS SGU/2 600 Z103081/00781 ECL 02.01 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  2.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345096_0192 W1345096/0192 ECL 1:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ: W1345096/0192 ECL 1
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0361 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/4521 ECL 2
- QNP-Accessory  : 1 X-input and 1 H-input

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20230420
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- 2HTX Amplifier: not available
- Lock: installed

SampleCase: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Automatic Changer: device connected to 149.236.99.252:/dev/tty04
- Capacity: 60 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 10 s
- Sample Rail fast changer mode = no

Cryo Controller CRCO: device connected to 149.236.99.252:/dev/tty01

Eurotherm VTU: device connected to 149.236.99.252:/dev/tty05

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                PN=Z003462, SN=00572 from 20071119
    Module  2 : XBB19F 2HS
                PN=Z003506, SN=00641 from 20071031
    Module  3 : 2H
                PN=Z003473, SN=00570 from 20071102



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0192 at TCP/IP 149.236.99.253)
SGU1 AUX  output -> open
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0192 at TCP/IP 149.236.99.253)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> open
SGU3 AUX  output -> input 3 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0192 at TCP/IP 149.236.99.253)
SGU4 NORM output -> input 4 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0192 at TCP/IP 149.236.99.253)
SGU4 AUX  output -> open

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAXH2H300/100/150 E 200-600MHZ W1345096/0192 at TCP/IP 149.236.99.253:
- amplifier 1H-100W uses blanking 2
- amplifier X-300W uses blanking 1
- amplifier 2H-150W needs no blanking


Switchbox (3 outputs: X / F / H) routing
--------------------------------------------------------------------
transmitter 1 = BLAXH2H300/100/150 E 200-600MHZ W1345096/0192 at TCP/IP 149.236.99.253:
- amplifier X-300W at blanking 1 can be routed to switchbox output 1 = X and output 2 = F
- amplifier 1H-100W at blanking 2 can be routed to switchbox output 1 = X, output 2 = F and output 3 = H
- amplifier 2H-150W can be routed to switchbox output 5 (unknown)


